# Change requests

## Spreadsheet: Redwells v0.32

## Requested by: Sandra

## Date 5th October 2020

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **Request** | **Change** | **Other consequences** | **Status** |
| 1 | Stop Thickness Needs Margins off 10mm - 50mm32 | Done | None |  |
| 2 | Stop Width Needs Margins Off 20mm - 250mm | Done | None |  |
| 3 | Timber Width Needs Margins Up to 250mm, anything over 197mm goes to 250mm timber | Already done in standard timber thickness table | None |  |
| 4 | Undercut Need To Be 3mm - 32mm | Done | None |  |
| 5 | Facings Width Margins 25mm - 120mm | Done | None |  |
| 6 | Facing Depth Margins 10mm - 35mm | Done | None |  |
| 7 | Frame Thickness Margins 15mm - 60mm | Done | None |  |
| 8 | -Frame Width Margins 50mm - 275mm | Done | None |  |
| 9 | Lintol Trench is 12mm if Timber is anything above 24mm or above, anything under 24mm to 18mm is a 7mm trench and anything under the 18mm is a 5mm trench option | Assumed “Timber” = lintol thickness. If lintol thickness is blank then still taking trench to be 12 mm. | None |  |
| 10 | Not every job needs an insert, can you either add an option to say None or add a N/A to the list please | Added checkbox for include inserts | Changed UpdateProgress to account for change in number of required fields |  |
| 11 | Can you add Ash timber to the list please. | Added. Need wholesale cost per cubic metre for ash and beech. | None |  |
| 12 | Can you change the Facings part please. Not every job has facing supplied but some jobs do require Thresholds supplied without baseblocks or facings. |  | None |  |
| 13 | The calculation for lintol is not correct the ( Example of 838 single, 838mm+6mm Width Clearance + 2xFrame Thickness (32mm) = 908mm, If double doorset it would be 142xdoor size(838+838) + 6mm Width Clearance + 3mm Meeting Style Clearance +2x Frame Thickness = 1749mm. | Corrected. | None |  |
| 14 | The Calculations for the leg should be ( Example - Door height (1981) + Undercut (28) + Head Clearance (3mm) + Trench (12mm) =2024mm. | No change needed. Error possibly a follow on from incorrect trench calculation | None |  |
| 15 | Basebloocks Thickness margins 10mm - 40mm | Done | None |  |
| 16 | Baseblocks Width Margins 30mm - 150mm  Done | Done | None |  |
| 17 | Baseblocks Height 75mm - 220mm | Done | None |  |
| 18 | Threshold Thickness 10mm - 40mm | Done | None |  |
| 19 | Threshold Width 35mm - 250mm | Done | None |  |
| 20 | Threshold Length 400mm - 2500mm | Done | None |  |

## Other comments

Still need min and max for lead door width, slave door width, door height, lintol thickness, insert width, insert depth.